**How to install your  Mounting Brackets**

**This guide shows the LDG series tuner but works for many items**

**You need a Rivet-Nut setting tool with 8/32 tip & aluminum nuts**

****

**DISASSEMBLE THE ITEM FOR PROPER SIZE RIVET NUT INSERTION**

****

**LOCATE THE ELECTRONICS AND AVOID INSTALLING THERE!**

**DRILL A HOLE IN EACH SIDE USING 17/64” DRILL BIT**

****

**MEASURE FOR DRILLING: 3.26” TO FRONT OR BACK AS THE HOLE WILL BE CENTERED**

****

**MEASURE TOP TO BOTTOM; CENTER THE HOLE LOCATION AND MARK FOR DRILLING HERE**

****

**INSERTING THE TOOL WITH 8-32” RIVET NUT ATTACHED, USE THIS SIZE FOR LDG TUNERS & GX5500 ROTOR CONTROL TOO**

****

**VIEW OF HOW THE RIVET NUT HOLE MISSES THE ELECTRONICS**

****

**FOR 90 DEGREE “L” BRACKET MOUNT LOOSELY ATTACH AND MARK IT**

****

****